6/7/2018

Placed a small thin teflon rectangle vertically in the sample rack, swept across from -5 degrees to 5 degrees under different laser angles, decided that it was best aligned when peak was minimized (maximally blocked by teflon).